{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Instructions and Properties","data","Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":17,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Instructions and Properties","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[[1,1,1,4],[2,1,2,4]]}
[]
[null,"!!!Macros must be enabled in order to utilize the functions included in this spreadsheet!!!"]
[null,"All temperatures are in Kelvin, option is only required/applies to saturated water and is to be specified as either liquid or vapor"]
[]
[null,null,"Material","Temperature (K)","Liquid or Gas"]
[null,null,"water",295,"Liquid"]
[null,"Property","Example Value","Function","Notes"]
[null,"Density (kg/m3)",{"$f":"rho(C6,D6,E6)","v":998.00399201596804},"rho(material, temperature, option)"]
[null,"Specific Heat (kJ/kg*K)",{"$f":"cp(C6,D6,E6)","v":4181},"cp(material, temperature, option)"]
[null,"Specific Entropy(kJ/kg)",{"$f":"hfg(C6,D6,E6)","v":2449000},"hfg(material, temperature, option)","available only for water, no option required"]
[null,"Dynamic Viscosity (N*s/m2)",{"$f":"mu(C6,D6,E6)","v":9.59E-4},"mu(material, temperature, option)"]
[null,"Kinematic Viscosity ( m2/s)",{"$f":"nu(C6,D6,E6)","v":9.6091800000000006E-7},"nu(material, temperature, option)"]
[null,"Conductive Coefficient (W/m*K)",{"$f":"k_val(C6,D6,E6)","v":0.60599999999999998},"k_val(material, temperature, option)"]
[null,"Alpha (m2/s)",{"$f":"alpha(C6,D6,E6)","v":1.4523128438172687E-7},"alpha(material, temperature, option)"]
[null,"Prandtl Number",{"$f":"pr(C6,D6,E6)","v":6.62},"Pr(material, temperature, option)"]
[null,"Surface Tension (N/m)",{"$f":"surf_ten(C6,D6,E6)","v":7.2700000000000001E-2},"surf_ten(material, temperatuare, option)","available only for liquid water, to option required"]
[null,"Beta(K-1)",{"$f":"Beta(C6,D6,E6)","v":2.275E-4},"Beta(material, temperature, option)"]
[]
[null,"Material and Option must be in \"\" if they are typed directly into the function.  If they are in cell that is referenced to the function, this is not necessary."]
[null,"For example you can write rho(\"water\", 312, \"liquid\") or rho(A12, A13, A14) where A12 is water, A13 is 312 and A14 is liquid."]
[]
[null,"You may use Sheet1 below or insert new sheets to perform calculations using these functions."]

{"sheet":"data","index":1,"n_rows":353,"n_cols":15,"rows_kept":353,"cut":false,"hidden":true,"merged":[]}
["air"]
["temp","rho","cp","mu","nu","k","alpha","Pr"]
[100,3.556,1032,7.1099999999999997E-6,1.9999999999999999E-6,9.3399999999999993E-3,2.5399999999999998E-6,0.78600000000000003]
[150,2.3359999999999999,1012,1.0339999999999999E-5,4.4259999999999996E-6,1.38E-2,5.84E-6,0.75800000000000001]
[200,1.746,1007,1.325E-5,7.5900000000000002E-6,1.8100000000000002E-2,1.03E-5,0.73699999999999999]
[250,1.395,1006,1.596E-5,1.1440000000000001E-5,2.23E-2,1.59E-5,0.72]
[300,1.161,1007,1.8459999999999999E-5,1.5889999999999999E-5,2.63E-2,2.2500000000000001E-5,0.70699999999999996]
[350,0.995,1009,2.0820000000000001E-5,2.092E-5,0.03,2.9899999999999998E-5,0.7]
[400,0.87109999999999999,1014,2.3010000000000002E-5,2.641E-5,3.3799999999999997E-2,3.8300000000000003E-5,0.69]
[450,0.77400000000000002,1021,2.5069999999999999E-5,3.239E-5,3.73E-2,4.7200000000000002E-5,0.68600000000000005]
[500,0.69640000000000002,1030,2.7010000000000001E-5,3.879E-5,4.07E-2,5.6700000000000003E-5,0.68400000000000005]
[550,0.63290000000000002,1040,2.8839999999999998E-5,4.5569999999999999E-5,4.3900000000000002E-2,6.6699999999999995E-5,0.68300000000000005]
[600,0.58040000000000003,1051,3.0580000000000002E-5,5.2689999999999999E-5,4.6899999999999997E-2,7.6899999999999999E-5,0.68500000000000005]
[650,0.53559999999999997,1063,3.2249999999999998E-5,6.0210000000000001E-5,4.9700000000000001E-2,8.7299999999999994E-5,0.69]
[700,0.4975,1075,3.3880000000000001E-5,6.8100000000000002E-5,5.2400000000000002E-2,9.7999999999999997E-5,0.69499999999999995]
[750,0.46429999999999999,1087,3.5460000000000003E-5,7.6370000000000002E-5,5.4899999999999997E-2,1.0900000000000001E-4,0.70199999999999996]
[800,0.43540000000000001,1099,3.6980000000000002E-5,8.4930000000000002E-5,5.7299999999999997E-2,1.2E-4,0.70899999999999996]
[850,0.40970000000000001,1110,3.8430000000000003E-5,9.3800000000000003E-5,5.96E-2,1.3100000000000001E-4,0.71599999999999997]
[900,0.38679999999999998,1121,3.981E-5,1.0289999999999999E-4,6.2E-2,1.4300000000000001E-4,0.72]
[950,0.36659999999999998,1131,4.1130000000000001E-5,1.122E-4,6.4299999999999996E-2,1.55E-4,0.72299999999999998]
[1000,0.34820000000000001,1141,4.244E-5,1.219E-4,6.6699999999999995E-2,1.6799999999999999E-4,0.72599999999999998]
[1100,0.31659999999999999,1159,4.49E-5,1.418E-4,7.1499999999999994E-2,1.95E-4,0.72799999999999998]
[1200,0.29020000000000001,1175,4.7299999999999998E-5,1.629E-4,7.6300000000000007E-2,2.24E-4,0.72799999999999998]
[1300,0.26790000000000003,1189,4.9599999999999999E-5,1.851E-4,8.2000000000000003E-2,2.3800000000000001E-4,0.71899999999999997]
[1400,0.24879999999999999,1207,5.3000000000000001E-5,2.13E-4,9.0999999999999998E-2,3.0299999999999999E-4,0.70299999999999996]
[1500,0.23219999999999999,1230,5.5699999999999999E-5,2.4000000000000001E-4,0.1,3.5E-4,0.68500000000000005]
[1600,0.2177,1248,5.8400000000000003E-5,2.6800000000000001E-4,0.106,3.8999999999999999E-4,0.68799999999999994]
[1700,0.2049,1267,6.1099999999999994E-5,2.9799999999999998E-4,0.113,4.35E-4,0.68500000000000005]
[1800,0.19350000000000001,1286,6.3700000000000003E-5,3.2899999999999997E-4,0.12,4.8200000000000001E-4,0.68300000000000005]
[1900,0.18329999999999999,1307,6.6299999999999999E-5,3.6200000000000002E-4,0.128,5.3399999999999997E-4,0.67700000000000005]
[2000,0.1741,1337,6.8899999999999994E-5,3.9599999999999998E-4,0.13700000000000001,5.8900000000000001E-4,0.67200000000000004]
[2100,0.1658,1372,7.1500000000000003E-5,4.3100000000000001E-4,0.14699999999999999,6.4599999999999998E-4,0.66700000000000004]
[2200,0.15820000000000001,1417,7.3999999999999996E-5,4.6799999999999999E-4,0.16,7.1400000000000001E-4,0.65500000000000003]
[2300,0.15129999999999999,1478,7.6600000000000005E-5,5.0600000000000005E-4,0.17499999999999999,7.8299999999999995E-4,0.64700000000000002]
[2400,0.14480000000000001,1558,7.9200000000000001E-5,5.4699999999999996E-4,0.19600000000000001,8.6899999999999998E-4,0.63]
[2500,0.1389,1665,8.1799999999999996E-5,5.8900000000000001E-4,0.222,9.6000000000000002E-4,0.61299999999999999]
[3000,0.1135,2726,9.5500000000000004E-5,8.4099999999999995E-4,0.48599999999999999,1.57E-3,0.53600000000000003]
[]
["nh3"]
["temp","rho","cp","mu","nu","k","alpha","Pr"]
[300,0.68940000000000001,2.1579999999999999,1.0149999999999999E-5,1.47E-5,2.47E-2,1.66E-5,0.88700000000000001]
[320,0.64480000000000004,2.17,1.0900000000000001E-5,1.6900000000000001E-5,2.7199999999999998E-2,1.9400000000000001E-5,0.87]
[340,0.60589999999999999,2.1920000000000002,1.165E-5,1.9199999999999999E-5,2.93E-2,2.2099999999999998E-5,0.872]
[360,0.5716,2.2210000000000001,1.24E-5,2.1699999999999999E-5,3.1600000000000003E-2,2.4899999999999999E-5,0.872]
[380,0.54100000000000004,2.254,1.31E-5,2.4199999999999999E-5,3.4000000000000002E-2,2.7900000000000001E-5,0.86899999999999999]
[400,0.51359999999999995,2.2869999999999999,1.38E-5,2.69E-5,3.6999999999999998E-2,3.15E-5,0.85299999999999998]
[420,0.48880000000000001,2.3220000000000001,1.45E-5,2.97E-5,4.0399999999999998E-2,3.5599999999999998E-5,0.83299999999999996]
[440,0.46639999999999998,2.3570000000000002,1.525E-5,3.2700000000000002E-5,4.3499999999999997E-2,3.96E-5,0.82599999999999996]
[460,0.44600000000000001,2.3929999999999998,1.59E-5,3.57E-5,4.6300000000000001E-2,4.3399999999999998E-5,0.82199999999999995]
[480,0.42730000000000001,2.4300000000000002,1.6650000000000002E-5,3.8999999999999999E-5,4.9200000000000001E-2,4.74E-5,0.82199999999999995]
[500,0.41010000000000002,2.4670000000000001,1.73E-5,4.2200000000000003E-5,5.2499999999999998E-2,5.1900000000000001E-5,0.81299999999999994]
[520,0.39419999999999999,2.504,1.8E-5,4.57E-5,5.45E-2,5.52E-5,0.82699999999999996]
[540,0.3795,2.54,1.8649999999999999E-5,4.9100000000000001E-5,5.7500000000000002E-2,5.9700000000000001E-5,0.82399999999999995]
[560,0.37080000000000002,2.577,1.9300000000000002E-5,5.1999999999999997E-5,6.0600000000000001E-2,6.3399999999999996E-5,0.82699999999999996]
[580,0.3533,2.613,1.995E-5,5.6499999999999998E-5,6.3799999999999996E-2,6.9099999999999999E-5,0.81699999999999995]
[]
["co2"]
["temp","rho","cp","mu","nu","k","alpha","Pr"]
[280,1.9021999999999999,0.83,1.4E-5,7.3599999999999998E-6,1.2500000000000001E-2,9.6299999999999993E-6,0.76500000000000001]
[300,1.7729999999999999,0.85099999999999998,1.49E-5,8.3999999999999992E-6,1.6549999999999999E-2,1.1E-5,0.76600000000000001]
[320,1.6609,0.872,1.56E-5,9.3899999999999999E-6,1.805E-2,1.2500000000000001E-5,0.754]
[340,1.5618000000000001,0.89100000000000001,1.6500000000000001E-5,1.06E-5,1.9699999999999999E-2,1.42E-5,0.746]
[360,1.4742999999999999,0.90800000000000003,1.73E-5,1.17E-5,2.12E-2,1.5800000000000001E-5,0.74099999999999999]
[380,1.3960999999999999,0.92600000000000005,1.7099999999999999E-5,1.2999999999999999E-5,2.2749999999999999E-2,1.7600000000000001E-5,0.73699999999999999]
[400,1.3257000000000001,0.94199999999999995,1.9000000000000001E-5,1.43E-5,2.4299999999999999E-2,1.95E-5,0.73699999999999999]
[450,1.1781999999999999,0.98099999999999998,2.0999999999999999E-5,1.7799999999999999E-5,2.8299999999999999E-2,2.4499999999999999E-5,0.72799999999999998]
[500,1.0593999999999999,1.02,2.3099999999999999E-5,2.1800000000000001E-5,3.2500000000000001E-2,3.01E-5,0.72499999999999998]
[550,0.96250000000000002,1.05,2.51E-5,2.6100000000000001E-5,3.6600000000000001E-2,3.6199999999999999E-5,0.72099999999999997]
[600,0.88260000000000005,1.08,2.6999999999999999E-5,3.0599999999999998E-5,4.07E-2,4.3800000000000001E-5,0.71699999999999997]
[650,0.81430000000000002,1.1000000000000001,2.8799999999999999E-5,3.54E-5,4.4499999999999998E-2,4.9700000000000002E-5,0.71199999999999997]
[700,0.75639999999999996,1.1299999999999999,3.0499999999999999E-5,4.0299999999999997E-5,4.8099999999999997E-2,5.63E-5,0.71699999999999997]
[750,0.70569999999999999,1.1499999999999999,3.2100000000000001E-5,4.5500000000000001E-5,5.1700000000000003E-2,6.3700000000000003E-5,0.71399999999999997]
[800,0.66139999999999999,1.17,3.3699999999999999E-5,5.1E-5,5.5100000000000003E-2,7.1199999999999996E-5,0.71599999999999997]
[]
["co"]
["temp","rho","cp","mu","nu","k","alpha","Pr"]
[200,1.6888000000000001,1.0449999999999999,1.27E-5,7.52E-6,1.7000000000000001E-2,9.6299999999999993E-6,0.78100000000000003]
[220,1.5341,1.044,1.3699999999999999E-5,8.9299999999999992E-6,1.9E-2,1.19E-5,0.753]
[240,1.4055,1.0429999999999999,1.47E-5,1.0499999999999999E-5,2.06E-2,1.4100000000000001E-5,0.74399999999999999]
[260,1.2967,1.0429999999999999,1.5699999999999999E-5,1.2099999999999999E-5,2.2100000000000002E-2,1.63E-5,0.74099999999999999]
[280,1.2038,1.042,1.66E-5,1.38E-5,2.3599999999999999E-2,1.88E-5,0.73299999999999998]
[300,1.1233,1.0429999999999999,1.7499999999999998E-5,1.56E-5,2.5000000000000001E-2,2.1299999999999999E-5,0.73]
[320,1.0528999999999999,1.0429999999999999,1.84E-5,1.7750000000000001E-5,2.63E-2,2.3900000000000002E-5,0.73]
[340,0.9909,1.044,1.9300000000000002E-5,1.95E-5,2.7799999999999998E-2,2.69E-5,0.72499999999999998]
[360,0.93569999999999998,1.0449999999999999,2.02E-5,2.16E-5,2.9100000000000001E-2,2.9799999999999999E-5,0.72499999999999998]
[380,0.88639999999999997,1.0469999999999999,2.0999999999999999E-5,2.37E-5,3.0499999999999999E-2,3.29E-5,0.71899999999999997]
[400,0.84209999999999996,1.0489999999999999,2.1800000000000001E-5,2.5899999999999999E-5,3.1800000000000002E-2,3.6000000000000001E-5,0.71899999999999997]
[450,0.74829999999999997,1.0549999999999999,2.37E-5,3.1699999999999998E-5,3.5000000000000003E-2,4.4299999999999999E-5,0.71399999999999997]
[500,0.67352000000000001,1.0649999999999999,2.5400000000000001E-5,3.7700000000000002E-5,3.8100000000000002E-2,5.3100000000000003E-5,0.71]
[550,0.61226000000000003,1.0760000000000001,2.7100000000000001E-5,4.4299999999999999E-5,4.1099999999999998E-2,6.2399999999999999E-5,0.71]
[600,0.56125999999999998,1.0880000000000001,2.8600000000000001E-5,5.1E-5,4.3999999999999997E-2,7.2100000000000004E-5,0.70699999999999996]
[650,0.51805999999999996,1.101,3.01E-5,5.8100000000000003E-5,4.7E-2,8.2399999999999997E-5,0.70499999999999996]
[700,0.48102,1.1140000000000001,3.15E-5,6.5500000000000006E-5,0.05,9.3300000000000005E-5,0.70199999999999996]
[750,0.44899,1.127,3.29E-5,7.3300000000000006E-5,5.28E-2,1.0399999999999999E-4,0.70199999999999996]
[800,0.42094999999999999,1.1399999999999999,3.43E-5,8.1500000000000002E-5,5.5500000000000001E-2,1.16E-4,0.70499999999999996]
[]
["he"]
["temp  ","rho   ","cp    ","mu","nu","k","alpha","Pr"]
[100,0.48709999999999998,0.51929999999999998,9.6299999999999993E-6,1.98E-5,7.2999999999999995E-2,2.8900000000000001E-5,0.68600000000000005]
[120,0.40600000000000003,0.51929999999999998,1.0699999999999999E-5,2.6400000000000001E-5,8.1900000000000001E-2,3.8800000000000001E-5,0.67900000000000005]
[140,0.34810000000000002,0.51929999999999998,1.1800000000000001E-5,3.3899999999999997E-5,9.0700000000000003E-2,5.02E-5,0.67600000000000005]
[160,0.30945,0.51929999999999998,1.29E-5,4.2599999999999999E-5,9.9199999999999997E-2,6.3200000000000005E-5,0.67449999999999999]
[180,0.27079999999999999,0.51929999999999998,1.3900000000000001E-5,5.13E-5,0.1072,7.6199999999999995E-5,0.67300000000000004]
[200,0.2462,0.51929999999999998,1.5E-5,6.1749999999999997E-5,0.11509999999999999,9.1600000000000004E-5,0.67400000000000004]
[220,0.22159999999999999,0.51929999999999998,1.5999999999999999E-5,7.2200000000000007E-5,0.1231,1.07E-4,0.67500000000000004]
[240,0.20455000000000001,0.51929999999999998,1.7E-5,8.4099999999999998E-5,0.13,1.2400000000000001E-4,0.67849999999999999]
[260,0.1875,0.51929999999999998,1.8E-5,9.6000000000000002E-5,0.13700000000000001,1.4100000000000001E-4,0.68200000000000005]
[280,0.17499999999999999,0.51929999999999998,1.9000000000000001E-5,1.0900000000000001E-4,0.14499999999999999,1.605E-4,0.68100000000000005]
[300,0.16250000000000001,0.51929999999999998,1.9899999999999999E-5,1.22E-4,0.152,1.8000000000000001E-4,0.68]
[350,0.14219999999999999,0.51929999999999998,2.2099999999999998E-5,1.605E-4,0.17,2.375E-4,0.67749999999999999]
[400,0.12189999999999999,0.51929999999999998,2.4300000000000001E-5,1.9900000000000001E-4,0.187,2.9500000000000001E-4,0.67500000000000004]
[450,0.10972,0.51929999999999998,2.6299999999999999E-5,2.4449999999999998E-4,0.20399999999999999,3.6450000000000002E-4,0.67149999999999999]
[500,9.7540000000000002E-2,0.51929999999999998,2.83E-5,2.9E-4,0.22,4.3399999999999998E-4,0.66800000000000004]
[550,9.0578000000000006E-2,0.51929999999999998,3.0150000000000001E-5,3.4299999999999999E-4,0.23599999999999999,5.1749999999999995E-4,0.66449999999999998]
[600,8.3614999999999995E-2,0.51929999999999998,3.1999999999999999E-5,3.9599999999999998E-4,0.252,6.0099999999999997E-4,0.66100000000000003]
[650,7.6652999999999999E-2,0.51929999999999998,3.3200000000000001E-5,4.4900000000000002E-4,0.26400000000000001,6.845E-4,0.65749999999999997]
[700,6.9690000000000002E-2,0.51929999999999998,3.4999999999999997E-5,5.0199999999999995E-4,0.27800000000000002,7.6800000000000002E-4,0.65400000000000003]
[750,6.6207000000000002E-2,0.51929999999999998,3.6399999999999997E-5,5.7067000000000001E-4,0.29099999999999998,8.7332999999999996E-4,0.65400000000000003]
[800,6.2723000000000001E-2,0.51929999999999998,3.82E-5,6.3933000000000002E-4,0.30399999999999999,9.7867000000000006E-4,0.65400000000000003]
[900,5.5757000000000001E-2,0.51929999999999998,4.1399999999999997E-5,7.7667000000000003E-4,0.33,1.1892999999999999E-3,0.65400000000000003]
[1000,4.879E-2,0.51929999999999998,4.46E-5,9.1399999999999999E-4,0.35399999999999998,1.4E-3,0.65400000000000003]
[]
["h2"]
["temp","rho","cp","mu","nu","k","alpha","Pr"]
[100,0.24254999999999999,11.23,4.2100000000000003E-6,1.7399999999999999E-5,6.7000000000000004E-2,2.4600000000000002E-5,0.70699999999999996]
[150,0.16156000000000001,12.6,5.5999999999999997E-6,3.4700000000000003E-5,0.10100000000000001,4.9599999999999999E-5,0.69899999999999995]
[200,0.12114999999999999,13.54,6.81E-6,5.6199999999999997E-5,0.13100000000000001,7.9900000000000004E-5,0.70399999999999996]
[250,9.6930000000000002E-2,14.06,7.8900000000000007E-6,8.14E-5,0.157,1.15E-4,0.70699999999999996]
[300,8.0780000000000005E-2,14.31,8.9600000000000006E-6,1.11E-4,0.183,1.5799999999999999E-4,0.70099999999999996]
[350,6.9239999999999996E-2,14.43,9.8800000000000003E-6,1.4300000000000001E-4,0.20399999999999999,2.04E-4,0.7]
[400,6.2590000000000007E-2,14.48,1.082E-5,1.7899999999999999E-4,0.22600000000000001,2.5799999999999998E-4,0.69499999999999995]
[450,5.3859999999999998E-2,14.5,1.172E-5,2.1800000000000001E-4,0.247,3.1599999999999998E-4,0.68899999999999995]
[500,4.8480000000000002E-2,14.52,1.2639999999999999E-5,2.61E-4,0.26600000000000001,3.7800000000000003E-4,0.69099999999999995]
[550,4.4069999999999998E-2,14.53,1.343E-5,3.0499999999999999E-4,0.28499999999999998,4.4499999999999997E-4,0.68500000000000005]
[600,4.0399999999999998E-2,14.55,1.4239999999999999E-5,3.5199999999999999E-4,0.30499999999999999,5.1900000000000004E-4,0.67800000000000005]
[700,3.4630000000000001E-2,14.61,1.5780000000000001E-5,4.5600000000000003E-4,0.34200000000000003,6.7599999999999995E-4,0.67500000000000004]
[800,3.1300000000000001E-2,14.7,1.7240000000000001E-5,5.6899999999999995E-4,0.378,8.4900000000000004E-4,0.67]
[900,2.6939999999999999E-2,14.83,1.8649999999999999E-5,6.9220000000000002E-4,0.41199999999999998,1.0300000000000001E-3,0.67100000000000004]
[1000,2.4240000000000001E-2,14.99,2.0129999999999999E-5,8.3000000000000001E-4,0.44800000000000001,1.23E-3,0.67300000000000004]
[1100,2.2040000000000001E-2,15.17,2.1299999999999999E-5,9.6599999999999995E-4,0.48799999999999999,1.4599999999999999E-3,0.66200000000000003]
[1200,2.0199999999999999E-2,15.37,2.262E-5,1.1199999999999999E-3,0.52800000000000002,1.6999999999999999E-3,0.65900000000000003]
[1300,1.865E-2,15.59,2.385E-5,1.279E-3,0.56799999999999995,1.9550000000000001E-3,0.65500000000000003]
[1400,1.7319999999999999E-2,15.81,2.5069999999999999E-5,1.4469999999999999E-3,0.61,2.2300000000000002E-3,0.65]
[1500,1.6160000000000001E-2,16.02,2.6270000000000001E-5,1.6260000000000001E-3,0.65500000000000003,2.5300000000000001E-3,0.64300000000000002]
[1600,1.52E-2,16.28,2.7370000000000001E-5,1.8010000000000001E-3,0.69699999999999995,2.8149999999999998E-3,0.63900000000000001]
[1700,1.43E-2,16.579999999999998,2.849E-5,1.9919999999999998E-3,0.74099999999999999,3.13E-3,0.63700000000000001]
[1800,1.35E-2,16.96,2.9609999999999999E-5,2.1930000000000001E-3,0.78600000000000003,3.4350000000000001E-3,0.63900000000000001]
[1900,1.2800000000000001E-2,17.489999999999998,3.0719999999999997E-5,2.3999999999999998E-3,0.83499999999999996,3.7299999999999998E-3,0.64300000000000002]
[2000,1.21E-2,18.25,3.1819999999999997E-5,2.63E-3,0.878,3.9750000000000002E-3,0.66100000000000003]
[]
["n2"]
["temp","rho","cp","mu","nu","k","alpha","Pr"]
[100,3.4388000000000001,1.07,6.8800000000000002E-6,1.9999999999999999E-6,9.58E-3,2.6000000000000001E-6,0.76800000000000002]
[150,2.2593999999999999,1.05,1.006E-5,4.4499999999999997E-6,1.3899999999999999E-2,5.8599999999999998E-6,0.75900000000000001]
[200,1.6882999999999999,1.0429999999999999,1.292E-5,7.6499999999999996E-6,1.83E-2,1.04E-5,0.73599999999999999]
[250,1.3488,1.042,1.5489999999999999E-5,1.148E-5,2.2200000000000001E-2,1.5800000000000001E-5,0.73699999999999999]
[300,1.1233,1.0409999999999999,1.7819999999999999E-5,1.5860000000000001E-5,2.5899999999999999E-2,2.2099999999999998E-5,0.71599999999999997]
[350,0.96250000000000002,1.042,2.0000000000000002E-5,2.0780000000000001E-5,2.93E-2,2.9200000000000002E-5,0.71099999999999997]
[400,0.84250000000000003,1.0449999999999999,2.2039999999999999E-5,2.616E-5,3.27E-2,3.7100000000000001E-5,0.70399999999999996]
[450,0.74850000000000005,1.05,2.3960000000000001E-5,3.201E-5,3.5799999999999998E-2,4.5599999999999997E-5,0.70299999999999996]
[500,0.67390000000000005,1.056,2.5769999999999999E-5,3.824E-5,3.8899999999999997E-2,5.4700000000000001E-5,0.7]
[550,0.61240000000000006,1.0649999999999999,2.747E-5,4.4860000000000001E-5,4.1700000000000001E-2,6.3899999999999995E-5,0.70199999999999996]
[600,0.5615,1.075,2.9079999999999999E-5,5.1789999999999997E-5,4.4600000000000001E-2,7.3899999999999994E-5,0.70099999999999996]
[700,0.48120000000000002,1.0980000000000001,3.2100000000000001E-5,6.6710000000000003E-5,4.99E-2,9.4400000000000004E-5,0.70599999999999996]
[800,0.42109999999999997,1.22,3.4910000000000003E-5,8.2899999999999996E-5,5.4800000000000001E-2,1.16E-4,0.71499999999999997]
[900,0.37430000000000002,1.1459999999999999,3.7530000000000002E-5,1.003E-4,5.9700000000000003E-2,1.3899999999999999E-4,0.72099999999999997]
[1000,0.33679999999999999,1.167,3.9990000000000002E-5,1.187E-4,6.4699999999999994E-2,1.56E-4,0.72099999999999997]
[1100,0.30620000000000003,1.1870000000000001,4.2320000000000001E-5,1.382E-4,7.0000000000000007E-2,1.93E-4,0.71799999999999997]
[1200,0.28070000000000001,1.204,4.4530000000000002E-5,1.5860000000000001E-4,7.5800000000000006E-2,2.24E-4,0.70699999999999996]
[1300,0.29509999999999997,1.2190000000000001,4.6619999999999997E-5,1.7990000000000001E-4,8.1000000000000003E-2,2.5599999999999999E-4,0.70099999999999996]
[]
["oxy"]
["temp","rho","cp","mu","nu","k","alpha","Pr"]
[100,3.9449999999999998,0.96199999999999997,7.6399999999999997E-6,1.9400000000000001E-6,9.2499999999999995E-3,2.4399999999999999E-6,0.79600000000000004]
[150,2.585,0.92100000000000004,1.148E-5,4.4399999999999998E-6,1.38E-2,5.8000000000000004E-6,0.76600000000000001]
[200,1.93,0.91500000000000004,1.4749999999999999E-5,7.6399999999999997E-6,1.83E-2,1.04E-5,0.73699999999999999]
[250,1.542,0.91500000000000004,1.7859999999999998E-5,1.1579999999999999E-5,2.2599999999999999E-2,1.5999999999999999E-5,0.72299999999999998]
[300,1.284,0.92,2.0720000000000002E-5,1.6140000000000001E-5,2.6800000000000001E-2,2.27E-5,0.71099999999999997]
[350,1.1000000000000001,0.92900000000000005,2.3349999999999998E-5,2.1229999999999998E-5,2.9600000000000001E-2,2.9E-5,0.73299999999999998]
[400,0.96199999999999997,0.94199999999999995,2.582E-5,2.6840000000000001E-5,3.3000000000000002E-2,3.6399999999999997E-5,0.73699999999999999]
[450,0.85540000000000005,0.95599999999999996,2.8140000000000002E-5,3.29E-5,3.6299999999999999E-2,4.4400000000000002E-5,0.74099999999999999]
[500,0.76980000000000004,0.97199999999999998,3.0329999999999999E-5,3.9400000000000002E-5,4.1200000000000001E-2,5.5099999999999998E-5,0.71599999999999997]
[550,0.69979999999999998,0.98799999999999999,3.2400000000000001E-5,4.6300000000000001E-5,4.41E-2,6.3800000000000006E-5,0.72599999999999998]
[600,0.64139999999999997,1.0029999999999999,3.4369999999999998E-5,5.359E-5,4.7300000000000002E-2,7.3499999999999998E-5,0.72899999999999998]
[700,0.54979999999999996,1.0309999999999999,3.8080000000000001E-5,6.9259999999999998E-5,5.28E-2,9.3700000000000001E-5,0.74399999999999999]
[800,0.48099999999999998,1.054,4.1510000000000001E-5,8.632E-5,5.8900000000000001E-2,1.16E-4,0.74299999999999999]
[900,0.42749999999999999,1.0740000000000001,4.4719999999999999E-5,1.0459999999999999E-4,6.4899999999999999E-2,1.4100000000000001E-4,0.74]
[1000,0.38479999999999998,1.0900000000000001,4.7700000000000001E-5,1.2400000000000001E-4,7.0999999999999994E-2,1.6899999999999999E-4,0.73299999999999998]
[1100,0.3498,1.103,5.0550000000000002E-5,1.4449999999999999E-4,7.5800000000000006E-2,1.9599999999999999E-4,0.73599999999999999]
[1200,0.3206,1.115,5.325E-5,1.661E-4,8.1900000000000001E-2,2.2900000000000001E-4,0.72499999999999998]
[1300,0.29599999999999999,1.125,5.8839999999999999E-5,1.886E-4,8.7099999999999997E-2,2.6200000000000003E-4,0.72099999999999997]
[]
["steam"]
["temp","rho","cp","mu","nu","k","alpha","Pr"]
[380,0.58630000000000004,2060,1.271E-5,2.1679999999999999E-5,2.46E-2,2.0400000000000001E-5,1.06]
[400,0.55420000000000003,2014,1.3339999999999999E-5,2.425E-5,2.6100000000000002E-2,2.34E-5,1.04]
[450,0.49020000000000002,1980,1.525E-5,3.1109999999999999E-5,2.9899999999999999E-2,3.0800000000000003E-5,1.01]
[500,0.4405,1985,1.7039999999999999E-5,3.8680000000000002E-5,3.39E-2,3.8800000000000001E-5,0.998]
[550,0.40050000000000002,1997,1.8839999999999999E-5,4.7039999999999997E-5,3.7900000000000003E-2,4.74E-5,0.99299999999999999]
[600,0.36520000000000002,2026,2.067E-5,5.66E-5,4.2200000000000001E-2,5.7000000000000003E-5,0.99299999999999999]
[650,0.33800000000000002,2056,2.247E-5,6.648E-5,4.6399999999999997E-2,6.6799999999999997E-5,0.996]
[700,0.314,2085,2.4260000000000002E-5,7.7260000000000002E-5,5.0500000000000003E-2,7.7100000000000004E-5,1]
[750,0.29310000000000003,2119,2.6040000000000001E-5,8.8839999999999996E-5,5.4899999999999997E-2,8.8399999999999994E-5,1]
[800,0.27389999999999998,2152,2.7860000000000001E-5,1.0170000000000001E-4,5.9200000000000003E-2,1E-4,1.01]
[850,0.25790000000000002,2186,2.9689999999999999E-5,1.1510000000000001E-4,6.3700000000000007E-2,1.13E-4,1.02]
[]
["oil"]
["temp","rho","cp","mu","nu","k","alpha","Pr","beta"]
[273,899.1,1796,3.85,4.28E-3,0.14699999999999999,9.0999999999999994E-8,47000,6.9999999999999999E-4]
[280,895.3,1827,2.17,2.4299999999999999E-3,0.14399999999999999,8.7999999999999994E-8,27500,6.9999999999999999E-4]
[290,890,1868,0.999,1.1199999999999999E-3,0.14499999999999999,8.72E-8,12900,6.9999999999999999E-4]
[300,884.1,1909,0.48599999999999999,5.5000000000000003E-4,0.14499999999999999,8.5899999999999995E-8,6400,6.9999999999999999E-4]
[310,877.9,1951,0.253,2.8800000000000001E-4,0.14499999999999999,8.4699999999999997E-8,3400,6.9999999999999999E-4]
[320,871.8,1993,0.14099999999999999,1.6100000000000001E-4,0.14299999999999999,8.2300000000000002E-8,1965,6.9999999999999999E-4]
[330,865.8,2035,8.3599999999999994E-2,9.6600000000000003E-5,0.14099999999999999,8.0000000000000002E-8,1205,6.9999999999999999E-4]
[340,859.9,2076,5.3100000000000001E-2,6.1699999999999995E-5,0.13900000000000001,7.7900000000000003E-8,793,6.9999999999999999E-4]
[350,853.9,2118,3.56E-2,4.1699999999999997E-5,0.13800000000000001,7.6300000000000002E-8,546,6.9999999999999999E-4]
[360,847.8,2161,2.52E-2,2.97E-5,0.13800000000000001,7.5300000000000006E-8,395,6.9999999999999999E-4]
[370,841.8,2206,1.8599999999999998E-2,2.1999999999999999E-5,0.13700000000000001,7.3799999999999999E-8,300,6.9999999999999999E-4]
[380,836,2250,1.41E-2,1.6900000000000001E-5,0.13600000000000001,7.2300000000000006E-8,233,6.9999999999999999E-4]
[390,830.6,2294,1.0999999999999999E-2,1.33E-5,0.13500000000000001,7.0900000000000006E-8,187,6.9999999999999999E-4]
[400,825.1,2337,8.7399999999999995E-3,1.06E-5,0.13400000000000001,6.9499999999999994E-8,152,6.9999999999999999E-4]
[410,818.9,2381,6.9800000000000001E-3,8.5199999999999997E-6,0.13300000000000001,6.8200000000000002E-8,125,6.9999999999999999E-4]
[420,812.1,2427,5.64E-3,6.9399999999999996E-6,0.13300000000000001,6.7500000000000002E-8,103,6.9999999999999999E-4]
[430,806.5,2471,4.7000000000000002E-3,5.8300000000000001E-6,0.13200000000000001,6.6199999999999997E-8,88,6.9999999999999999E-4]
[]
["ethyl_gly"]
["temp","rho","cp","mu","nu","k","alpha","Pr","beta"]
[273,1131,2294,6.5100000000000005E-2,5.7599999999999997E-5,0.24199999999999999,9.3299999999999995E-8,617,6.4999999999999997E-4]
[280,1126,2323,4.2000000000000003E-2,3.7299999999999999E-5,0.24399999999999999,9.3299999999999995E-8,400,6.4999999999999997E-4]
[290,1119,2368,2.47E-2,2.2099999999999998E-5,0.248,9.3600000000000004E-8,236,6.4999999999999997E-4]
[300,1114,2415,1.5699999999999999E-2,1.4100000000000001E-5,0.252,9.39E-8,151,6.4999999999999997E-4]
[310,1104,2460,1.0699999999999999E-2,9.6500000000000008E-6,0.255,9.39E-8,103,6.4999999999999997E-4]
[320,1096,2505,7.5700000000000003E-3,6.9099999999999999E-6,0.25800000000000001,9.3999999999999995E-8,73.5,6.4999999999999997E-4]
[330,1090,2549,5.6100000000000004E-3,5.1499999999999998E-6,0.26,9.3600000000000004E-8,55,6.4999999999999997E-4]
[340,1084,2592,4.3099999999999996E-3,3.98E-6,0.26100000000000001,9.2900000000000005E-8,42.8,6.4999999999999997E-4]
[350,1079,2637,3.4199999999999999E-3,3.1700000000000001E-6,0.26100000000000001,9.1699999999999994E-8,34.6,6.4999999999999997E-4]
[360,1074,2682,2.7799999999999999E-3,2.5900000000000002E-6,0.26100000000000001,9.0600000000000004E-8,28.6,6.4999999999999997E-4]
[370,1067,2728,2.2799999999999999E-3,2.1399999999999998E-6,0.26200000000000001,8.9999999999999999E-8,23.7,6.4999999999999997E-4]
[373,1059,2742,2.15E-3,2.03E-6,0.26300000000000001,9.0600000000000004E-8,22.4,6.4999999999999997E-4]
[]
["glyc fluid"]
["temp","rho      ","cp       ","mu       ","nu       ","k        ","alpha    ","Pr       ","beta     "]
[273,1276,2261,10.6,8.3099999999999997E-3,0.28199999999999997,9.7699999999999995E-8,85000,4.6999999999999999E-4]
[280,1271.9000000000001,2298,5.34,4.1999999999999997E-3,0.28399999999999997,9.7199999999999997E-8,43200,4.6999999999999999E-4]
[290,1265.8,2367,1.85,1.4599999999999999E-3,0.28599999999999998,9.5500000000000002E-8,15300,4.8000000000000001E-4]
[300,1259.9000000000001,2427,0.79900000000000004,6.3400000000000001E-4,0.28599999999999998,9.3499999999999997E-8,6780,4.8000000000000001E-4]
[310,1253.9000000000001,2490,0.35199999999999998,2.81E-4,0.28599999999999998,9.16E-8,3060,4.8999999999999998E-4]
[320,1247.2,2564,0.21,1.6799999999999999E-4,0.28699999999999998,8.9700000000000003E-8,1870,5.0000000000000001E-4]
[]
["r132a fluid"]
["temp     ","rho      ","cp       ","mu       ","nu       ","k        ","alpha    ","Pr       ","beta     "]
[230,1426.8,1.2490000000000001,4.9120000000000001E-4,3.3430000000000002E-7,0.11210000000000001,6.2900000000000001E-8,5.5,2.0200000000000001E-3]
[240,1397.7,1.2669999999999999,4.2020000000000002E-4,3.0059999999999998E-7,0.10730000000000001,6.06E-8,5,2.1099999999999999E-3]
[250,1367.9,1.2869999999999999,3.6329999999999999E-4,2.656E-7,0.10249999999999999,5.8299999999999999E-8,4.5999999999999996,2.2300000000000002E-3]
[260,1337.1,1.3080000000000001,3.166E-4,2.368E-7,9.7900000000000001E-2,5.5999999999999999E-8,4.2,2.3600000000000001E-3]
[270,1305.0999999999999,1.333,2.7750000000000002E-4,2.1269999999999999E-7,9.3399999999999997E-2,5.3699999999999998E-8,4,2.5300000000000001E-3]
[280,1271.8,1.361,2.4429999999999998E-4,1.9210000000000001E-7,8.8999999999999996E-2,5.1399999999999997E-8,3.7,2.7299999999999998E-3]
[290,1236.8,1.393,2.1560000000000001E-4,1.744E-7,8.4599999999999995E-2,4.9100000000000003E-8,3.5,2.98E-3]
[300,1199.7,1.4319999999999999,1.905E-4,1.5879999999999999E-7,8.0299999999999996E-2,4.6800000000000002E-8,3.4,3.3E-3]
[310,1159.9000000000001,1.4810000000000001,1.6799999999999999E-4,1.4490000000000001E-7,7.6100000000000001E-2,4.43E-8,3.3,3.7299999999999998E-3]
[320,1116.8,1.5429999999999999,1.4779999999999999E-4,1.3229999999999999E-7,7.1800000000000003E-2,4.1700000000000003E-8,3.2,4.3299999999999996E-3]
[330,1069.0999999999999,1.627,1.292E-4,1.209E-7,6.7500000000000004E-2,3.8799999999999997E-8,3.1,5.1900000000000002E-3]
[340,1015,1.7509999999999999,1.1179999999999999E-4,1.1019999999999999E-7,6.3100000000000003E-2,3.55E-8,3.1,6.5700000000000003E-3]
[350,951.3,1.9610000000000001,8.5099999999999995E-5,9.9999999999999995E-8,5.8599999999999999E-2,3.1400000000000003E-8,3.2,9.1000000000000004E-3]
[360,870.1,2.4369999999999998,7.8100000000000001E-5,8.9799999999999997E-8,5.4100000000000002E-2,2.55E-8,3.5,1.5389999999999999E-2]
[370,740.3,5.1050000000000004,5.8E-5,7.8300000000000006E-8,5.1799999999999999E-2,1.37E-8,5.7,5.5239999999999997E-2]
[]
["R22 fluid"]
["temp     ","rho      ","cp       ","mu       ","nu       ","k        ","alpha    ","Pr       ","beta     "]
[230,1416,1.087,3.5579999999999997E-4,2.5129999999999998E-7,0.1145,7.4400000000000004E-8,3.4,2.0500000000000002E-3]
[240,1386.6,1.1000000000000001,3.145E-4,2.2670000000000001E-7,0.10979999999999999,7.1999999999999996E-8,3.2,2.16E-3]
[250,1356.3,1.117,2.7960000000000002E-4,2.0620000000000001E-7,0.1052,6.9499999999999994E-8,3,2.2899999999999999E-3]
[260,1324.9,1.137,2.497E-4,1.8839999999999999E-7,0.1007,6.6800000000000003E-8,2.8,2.4499999999999999E-3]
[270,1292.0999999999999,1.161,2.2350000000000001E-4,1.73E-7,9.6199999999999994E-2,6.4099999999999998E-8,2.7,2.63E-3]
[280,1257.9000000000001,1.1890000000000001,2.0049999999999999E-4,1.5940000000000001E-7,9.1700000000000004E-2,6.13E-8,2.6,2.8600000000000001E-3]
[290,1221.7,1.2230000000000001,1.7980000000000001E-4,1.4719999999999999E-7,8.72E-2,5.8299999999999999E-8,2.5,3.15E-3]
[300,1183.4000000000001,1.2649999999999999,1.6100000000000001E-4,1.3610000000000001E-7,8.2600000000000007E-2,5.5199999999999998E-8,2.5,3.5100000000000001E-3]
[310,1142.2,1.319,1.438E-4,1.2590000000000001E-7,7.8100000000000003E-2,5.1800000000000001E-8,2.4,4.0000000000000001E-3]
[320,1097.4000000000001,1.391,1.2779999999999999E-4,1.165E-7,7.3400000000000007E-2,4.8100000000000001E-8,2.4,4.6899999999999997E-3]
[330,1047.5,1.4950000000000001,1.127E-4,1.075E-7,6.8599999999999994E-2,4.3800000000000002E-8,2.5,5.7499999999999999E-3]
[340,990.1,1.665,9.7999999999999997E-5,9.8900000000000005E-8,6.3600000000000004E-2,3.8600000000000002E-8,2.6,7.5599999999999999E-3]
[350,920.1,1.9970000000000001,8.3100000000000001E-5,9.0400000000000002E-8,5.8299999999999998E-2,3.1699999999999999E-8,2.8,1.1350000000000001E-2]
[360,823.4,3.0009999999999999,6.6799999999999997E-5,8.1100000000000005E-8,5.3100000000000001E-2,2.1500000000000001E-8,3.8,2.3879999999999998E-2]
[]
["hg fluid"]
["temp","rho      ","    cp      ","    mu       ","nu       ","k        ","alpha    ","Pr       ","beta     "]
[273,13595,140.4,1.688E-3,1.24E-7,8.18,4.2849999999999996E-6,2.9000000000000001E-2,1.8100000000000001E-4]
[300,13529,139.30000000000001,1.523E-3,1.1249999999999999E-7,8.5399999999999991,4.5299999999999998E-6,2.4799999999999999E-2,1.8100000000000001E-4]
[350,13407,137.69999999999999,1.3090000000000001E-3,9.76E-8,9.18,4.9749999999999998E-6,1.9599999999999999E-2,1.8100000000000001E-4]
[400,13287,136.5,1.1709999999999999E-3,8.8199999999999996E-8,9.8000000000000007,5.4049999999999999E-6,1.6299999999999999E-2,1.8100000000000001E-4]
[450,13167,135.69999999999999,1.075E-3,8.1600000000000003E-8,10.4,5.8100000000000003E-6,1.4E-2,1.8100000000000001E-4]
[500,13048,135.30000000000001,1.0070000000000001E-3,7.7099999999999996E-8,10.95,6.19E-6,1.2500000000000001E-2,1.8200000000000001E-4]
[550,12929,135.19999999999999,9.5299999999999996E-4,7.3700000000000005E-8,11.45,6.5549999999999999E-6,1.12E-2,1.84E-4]
[600,12809,135.5,9.1100000000000003E-4,7.1099999999999995E-8,11.95,6.8800000000000002E-6,1.03E-2,1.8699999999999999E-4]
[]
["water fluid"]
["temp","pressure","vf","vg","hfg","cpf","cpg","muf","mug","kf","kg","prf","prg","sigma    ","beta "]
[273.14999999999998,611,1E-3,206.3,2502000,4217,1854,1.75E-3,8.0199999999999994E-6,0.56899999999999995,1.8200000000000001E-2,12.99,0.81499999999999995,7.5499999999999998E-2,-6.8050000000000001E-5]
[275,697,1E-3,181.7,2497000,4211,1855,1.652E-3,8.0900000000000005E-6,0.57399999999999995,1.83E-2,12.22,0.81699999999999995,7.5300000000000006E-2,-3.2740000000000002E-5]
[280,990,1E-3,130.4,2485000,4198,1858,1.4220000000000001E-3,8.2900000000000002E-6,0.58199999999999996,1.8599999999999998E-2,10.26,0.82499999999999996,7.4800000000000005E-2,4.604E-5]
[285,1387,1E-3,99.4,2473000,4189,1861,1.225E-3,8.49E-6,0.59,1.89E-2,8.81,0.83299999999999996,7.4300000000000005E-2,1.141E-4]
[290,1917,1.0009999999999999E-3,69.7,2461000,4184,1864,1.08E-3,8.6899999999999998E-6,0.59799999999999998,1.9300000000000001E-2,7.56,0.84099999999999997,7.3700000000000002E-2,1.74E-4]
[295,2617,1.0020000000000001E-3,51.94,2449000,4181,1868,9.59E-4,8.8899999999999996E-6,0.60599999999999998,1.95E-2,6.62,0.84899999999999998,7.2700000000000001E-2,2.275E-4]
[300,3531,1.003E-3,39.130000000000003,2438000,4179,1872,8.5499999999999997E-4,9.0899999999999994E-6,0.61299999999999999,1.9599999999999999E-2,5.83,0.85699999999999998,7.17E-2,2.7609999999999999E-4]
[305,4712,1.005E-3,29.74,2426000,4178,1877,7.6900000000000004E-4,9.2900000000000008E-6,0.62,2.01E-2,5.2,0.86499999999999999,7.0900000000000005E-2,3.2059999999999999E-4]
[310,6221,1.0070000000000001E-3,22.93,2414000,4178,1882,6.9499999999999998E-4,9.4900000000000006E-6,0.628,2.0400000000000001E-2,4.62,0.873,7.0000000000000007E-2,3.6190000000000001E-4]
[315,8132,1.0089999999999999E-3,17.82,2402000,4179,1888,6.3100000000000005E-4,9.6900000000000004E-6,0.63400000000000001,2.07E-2,4.16,0.88300000000000001,6.9199999999999998E-2,4.0039999999999997E-4]
[320,10530,1.011E-3,13.98,2390000,4180,1895,5.7700000000000004E-4,9.8900000000000002E-6,0.64,2.1000000000000001E-2,3.77,0.89400000000000002,6.83E-2,4.3669999999999999E-4]
[325,13510,1.013E-3,11.06,2378000,4182,1903,5.2800000000000004E-4,1.009E-5,0.64500000000000002,2.1299999999999999E-2,3.42,0.90100000000000002,6.7500000000000004E-2,4.7120000000000002E-4]
[330,17190,1.016E-3,8.82,2366000,4184,1911,4.8899999999999996E-4,1.029E-5,0.65,2.1700000000000001E-2,3.15,0.90800000000000003,6.6600000000000006E-2,5.04E-4]
[335,21670,1.018E-3,7.09,2354000,4186,1920,4.5300000000000001E-4,1.049E-5,0.65600000000000003,2.1999999999999999E-2,2.88,0.91600000000000004,6.5799999999999997E-2,5.3549999999999995E-4]
[340,27130,1.021E-3,5.74,2342000,4188,1930,4.2000000000000002E-4,1.0689999999999999E-5,0.66,2.23E-2,2.66,0.92500000000000004,6.4899999999999999E-2,5.6599999999999999E-4]
[345,33720,1.024E-3,4.6829999999999998,2329000,4191,1941,3.8900000000000002E-4,1.0890000000000001E-5,0.66800000000000004,2.2599999999999999E-2,2.4500000000000002,0.93300000000000005,6.4100000000000004E-2,5.9540000000000005E-4]
[350,41630,1.0269999999999999E-3,3.8460000000000001,2317000,4195,1954,3.6499999999999998E-4,1.1090000000000001E-5,0.66800000000000004,2.3E-2,2.29,0.94199999999999995,6.3200000000000006E-2,6.2419999999999999E-4]
[355,51000,1.0300000000000001E-3,3.18,2304000,4199,1968,3.4299999999999999E-4,1.129E-5,0.67100000000000004,2.3300000000000001E-2,2.14,0.95099999999999996,6.2300000000000001E-2,6.5229999999999997E-4]
[360,62090,1.034E-3,2.645,2291000,4203,1983,3.2400000000000001E-4,1.149E-5,0.67400000000000004,2.3699999999999999E-2,2.02,0.96,6.1400000000000003E-2,6.979E-4]
[365,75140,1.0380000000000001E-3,2.2120000000000002,2278000,4209,1999,3.0600000000000001E-4,1.169E-5,0.67700000000000005,2.41E-2,1.91,0.96899999999999997,6.0499999999999998E-2,7.071E-4]
[370,90400,1.041E-3,1.861,2265000,4214,2017,2.8899999999999998E-4,1.189E-5,0.67900000000000005,2.4500000000000001E-2,1.8,0.97799999999999998,5.9499999999999997E-2,7.2869999999999999E-4]
[373.15,101300,1.044E-3,1.679,2257000,4217,2029,2.7900000000000001E-4,1.202E-5,0.68,2.4799999999999999E-2,1.76,0.98399999999999999,5.8900000000000001E-2,7.5009999999999996E-4]
[375,108200,1.0449999999999999E-3,1.5740000000000001,2252000,4220,2036,2.7399999999999999E-4,1.2089999999999999E-5,0.68100000000000005,2.4899999999999999E-2,1.7,0.98699999999999999,5.8599999999999999E-2,7.6099999999999996E-4]
[380,128700,1.049E-3,1.337,2239000,4226,2057,2.5999999999999998E-4,1.2289999999999999E-5,0.68300000000000005,2.5399999999999999E-2,1.61,0.999,5.7599999999999998E-2,7.8799999999999996E-4]
[385,152300,1.0529999999999999E-3,1.1419999999999999,2225000,4232,2080,2.4800000000000001E-4,1.2490000000000001E-5,0.68500000000000005,2.58E-2,1.53,1.004,5.6599999999999998E-2,8.1400000000000005E-4]
[390,179400,1.0579999999999999E-3,0.98,2212000,4239,2104,2.3699999999999999E-4,1.269E-5,0.68600000000000005,2.63E-2,1.47,1.0129999999999999,5.5599999999999997E-2,8.4099999999999995E-4]
[400,245500,1.067E-3,0.73099999999999998,2183000,4256,2158,2.1699999999999999E-4,1.305E-5,0.68799999999999994,2.7199999999999998E-2,1.34,1.0329999999999999,5.3600000000000002E-2,8.9599999999999999E-4]
[410,330200,1.077E-3,0.55300000000000005,2153000,4278,2221,2.0000000000000001E-4,1.342E-5,0.68799999999999994,2.8199999999999999E-2,1.24,1.054,5.1499999999999997E-2,9.5200000000000005E-4]
[420,437000,1.088E-3,0.42499999999999999,2123000,4302,2291,1.85E-4,1.379E-5,0.68799999999999994,2.98E-2,1.1599999999999999,1.075,4.9399999999999999E-2,1.01E-3]
[430,569900,1.0989999999999999E-3,0.33100000000000002,2091000,4331,2369,1.73E-4,1.414E-5,0.68500000000000005,3.04E-2,1.0900000000000001,1.1000000000000001,4.7199999999999999E-2]
[440,733300,1.1100000000000001E-3,0.26100000000000001,2059000,4360,2460,1.6200000000000001E-4,1.45E-5,0.68200000000000005,3.1699999999999999E-2,1.04,1.1200000000000001,4.5100000000000001E-2]
[450,931900,1.1230000000000001E-3,0.20799999999999999,2024000,4400,2560,1.5200000000000001E-4,1.485E-5,0.67800000000000005,3.3099999999999997E-2,0.99,1.1399999999999999,4.2900000000000001E-2]
[460,1171000,1.137E-3,0.16700000000000001,1989000,4440,2680,1.4300000000000001E-4,1.519E-5,0.67300000000000004,3.4599999999999999E-2,0.95,1.17,4.07E-2]
[470,1455000,1.152E-3,0.13600000000000001,1951000,4480,2790,1.36E-4,1.554E-5,0.66700000000000004,3.6299999999999999E-2,0.92,1.2,3.85E-2]
[480,1790000,1.1670000000000001E-3,0.111,1912000,4530,2940,1.2899999999999999E-4,1.588E-5,0.66,3.8100000000000002E-2,0.89,1.23,3.6200000000000003E-2]
[490,2183000,1.1839999999999999E-3,9.2200000000000004E-2,1870000,4590,3100,1.2400000000000001E-4,1.6229999999999999E-5,0.65100000000000002,4.0099999999999997E-2,0.87,1.25,3.39E-2]
[500,2640000,1.2030000000000001E-3,7.6600000000000001E-2,1825000,4660,3270,1.18E-4,1.6589999999999999E-5,0.64200000000000002,4.2299999999999997E-2,0.86,1.28,3.1600000000000003E-2]
[510,3166000,1.222E-3,6.3100000000000003E-2,1779000,4740,3470,1.13E-4,1.6949999999999999E-5,0.63100000000000001,4.4699999999999997E-2,0.85,1.31,2.93E-2]
[520,3770000,1.2440000000000001E-3,5.2499999999999998E-2,1730000,4840,3700,1.08E-4,1.7329999999999998E-5,0.621,4.7500000000000001E-2,0.84,1.35,2.69E-2]
[530,4458000,1.268E-3,4.4499999999999998E-2,1679000,4950,3960,1.0399999999999999E-4,1.772E-5,0.60799999999999998,5.0599999999999999E-2,0.85,1.39,2.4500000000000001E-2]
[540,5238000,1.294E-3,3.7499999999999999E-2,1622000,5080,4270,1.01E-4,1.8099999999999999E-5,0.59399999999999997,5.3999999999999999E-2,0.86,1.43,2.2100000000000002E-2]
[550,6119000,1.323E-3,3.1699999999999999E-2,1564000,5240,4640,9.7E-5,1.8600000000000001E-5,0.57999999999999996,5.8299999999999998E-2,0.87,1.47,1.9699999999999999E-2]
[560,7108000,1.3550000000000001E-3,2.69E-2,1499000,5430,5090,9.3999999999999994E-5,1.91E-5,0.56299999999999994,6.3700000000000007E-2,0.9,1.52,1.7299999999999999E-2]
[570,8216000,1.392E-3,2.2800000000000001E-2,1429000,5680,5670,9.1000000000000003E-5,1.9700000000000001E-5,0.54800000000000004,7.6700000000000004E-2,0.94,1.59,1.4999999999999999E-2]
[580,9451000,1.433E-3,1.9300000000000001E-2,1353000,6000,6400,8.7999999999999998E-5,2.0400000000000001E-5,0.52800000000000002,7.6700000000000004E-2,0.99,1.68,1.2800000000000001E-2]
[590,10830000,1.482E-3,1.6299999999999999E-2,1274000,6410,7350,8.3999999999999995E-5,2.1500000000000001E-5,0.51300000000000001,8.4099999999999994E-2,1.05,1.84,1.0500000000000001E-2]
[600,12350000,1.5410000000000001E-3,1.37E-2,1176000,7000,8750,8.1000000000000004E-5,2.27E-5,0.497,9.2899999999999996E-2,1.1399999999999999,2.15,8.3999999999999995E-3]
[610,13730000,1.6119999999999999E-3,1.15E-2,1068000,7850,11100,7.7000000000000001E-5,2.41E-5,0.46700000000000003,0.10299999999999999,1.3,2.6,6.3E-3]
[620,15910000,1.7049999999999999E-3,9.4000000000000004E-3,941000,9350,15400,7.2000000000000002E-5,2.5899999999999999E-5,0.44400000000000001,0.114,1.52,3.46,4.4999999999999997E-3]
[625,16910000,1.7780000000000001E-3,8.5000000000000006E-3,858000,10600,18300,6.9999999999999994E-5,2.6999999999999999E-5,0.43,0.121,1.65,4.2,3.5000000000000001E-3]
[630,17970000,1.856E-3,7.4999999999999997E-3,781000,12600,22100,6.7000000000000002E-5,2.8E-5,0.41199999999999998,0.13,2,4.8,2.5999999999999999E-3]
[635,19090000,1.9350000000000001E-3,6.6E-3,683000,16400,27600,6.3999999999999997E-5,3.0000000000000001E-5,0.39200000000000002,0.14099999999999999,2.7,6,1.5E-3]
[640,20270000,2.075E-3,5.7000000000000002E-3,560000,26000,42000,5.8999999999999998E-5,3.1999999999999999E-5,0.36699999999999999,0.155,4.2,9.6,8.0000000000000004E-4]
[645,21520000,2.3509999999999998E-3,4.4999999999999997E-3,361000,90000,null,5.3999999999999998E-5,3.6999999999999998E-5,0.33100000000000002,0.17799999999999999,12,26,1E-4]
[647.29999999999995,22120000,3.1700000000000001E-3,3.2000000000000002E-3,0,"inf","inf",4.5000000000000003E-5,4.5000000000000003E-5,0.23799999999999999,0.23799999999999999,"inf","inf",0]

{"sheet":"Sheet1","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}